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Protocol Description

This protocol contains 9 types of packet frames.

Command:


"A253|_||_|" or "A<DID>|_||_|"  
Read node Address

"A253|_|" or "A<DID>|_|"  

Set node ID (0x01...0xFE)


"V<DID>|_|xxxx|_|" 
Set HV "high voltage". HV changes between                

900 - 2500 volt

"E<DID>|_|xxxx|_|" 
Set HV in ADC units


"H<DID>|_|" 
Request to HV to get voltage


"R<DID>|_|" 
Request and Read HV in ADC units


"G<DID>|_|" 
Switch on HV


"S<DID>|_|" 
Switch off HV


"C<DID>|_|xxxx|_|" 
Calibrate HV

*notes:



<DID> - Address of destination node.


|_| - Space
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